**Ultra Sonic Cool Mist Humidifier**

*Last revised June 5, 2024*

# **Purpose**

# The purpose of this standard operating procedure is to define the proper use, maintenance and standards required of the Ultra Sonic Cool Mist humidifier utilized by the Lab Animal Resources Department.

# **Responsibility**

# It is the responsibility of all animal users, including investigators, their technicians and LAR to properly use and maintain the Ultra Sonic Cool Mist Humidifier in order to provide the require levels of humidity in the animal room(s).

**Basic info**

The humidifier uses ultrasonic waves to generate 1.7 million high frequency oscillations per second. The water is atomized into ultra-fine particles of 1 to 5 microns, and the water mist is diffused to the air through the air moving device. Thereby achieving the purpose of evenly humidifying the air. The humidifier keeps the room at the desired humidity and prevents static electricity.

# **Instructions for Use**

Check that unit is in good working order and all the parts are accounted for. Lift the main body and put the water pump at the bottom of the tank, make sure to place it in a balances, horizontal position.

Top fill the water, making sure not to exceed the maxium water level.

Add white mist tube on to the top cover

Plug in the power cord

A beep will sound at the same time

The machine will automatically enter standby state

Press On/Off to turn on

The machine will start to work at the default highest mist volume. Until otherwise set.

**Additional Features**

Sleep mode

Press On/off for 3 seconds to enter sleep mode and the display will go out.

Touch again to turn off the sleep mode

Mist Volume

1/2/3/4 – low/medium/high/highest

4 mist volume levels are adjustable by pressing he button

The numbers (1/2/3/4) will flash on the screen to indicate which level the mist is on

Intermittent Mist

1M/3M/5M will flash on the screen

It has 4 options

1M – mist for 1 minute then stop for 1 minute

3M – mist for 1 minute then stop for 3 minutes

5M – mist for 1 minute then stop for 5 minutes

Continuously Mist – press until the signals of 1M/3M/5M goes out

Timer

88H flashes

Timer can be set from 00H to 16H

Adjust 1 hour per touch

Touch the button to activate the timing adjustment and 00H will flash on the screen. If the timer setting is finished then the number value will flash 5 times

When the preset timer is reached the machine will automatically shut off

Customize Humidity

You can customize the desired humidity levels from 45% to 95 %

Touch the button for 1st time to activate the constant humidity function and the humidity value will keep flashing.

If the adjustment stops the machine will work according to the current humidity value

Touch the button a 2nd time ti adjust the preset humidity leels

It adjusts 5% room humidity (RH) per touch

The maximum humidity level setting is 95%, touch once more to turn off the humididty setting

Once the machine has reached the preset desired room humidity level it will stop. When the room humidity falls below the preset value the machine will turn on again to reach the setting

UV lamp

Touch the button to activate the UV lamp function

Signal of the UV lamp lights up and flashes

Touch again to turn off

Essential Oil Tray

Press the tray at the back of the humidifier, it will pop out. The silicone and sponge cover inside will last the lifetime of the machine.

The manual recommends to only use 2 drops of essential oil.

It is not recommended to NOT use essential oils in LAR facilities

# **Safety Guide**

# **Common Problems and Solutions**

# **Routine Maintenance**

# **Notes + Tips**